,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Lunexo H2 CDP-I 8800 840 ETDD 03,1.503,0.2,0.045,10143003;,6826051;,Lunexo_H_GH,Weißaluminium RAL 9006;,10.5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6826051,Schutzklasse I;,IP20;,ETDD,LED,80,80,8.298,4000,TRILUX_Alu_RAL_9006,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX050921
