,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,PrimEqui##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,MatSupEqui##OTHER##,SEO##OTHER##,Light Source##OTHER##
ArimoFit Act M46 DW19 42-8 ETDD8 (ActDSU),1.197,0.297,0.02,10216423,7523762,ArimoFit_M46_ M48_M57_M59_M73_M84,ArimoFit_no_accessories,RAL9016 Verkehrsweiß,3.6,http://www.trilux.com/TOC/7523762,I,IP40,ETDD8,LED,40,80,62 88 98 100 100 0 0 0 0,4200,4000,TRILUX_RAL9016,TRILUX_RAL9016,TRILUX_WH_4000,ArimoFit_LS : TX149815
