,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,RegPrim##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
LunexoAct D2 CDP-I 5500 ETDD8 +LLWC 01 ACTDCW,1.503, 0.2, 0.049,10248282,7793462,RAL9016 Verkehrsweiß, 10.5,http://www.trilux.com/TOC/7793462,I,IP20,ETDD8,LED,59,80,60 88 98 99 100 0 0 50 1,5500,6100,Lunexo_D_GH,TRILUX_RAL9016,TRILUX_WH_6100,Lunexo_LS : TX277622
