,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
CreavoAct M48-TS LWW-03 53-8 ETDD8 01 (ActDCW),1.497,0.297,0.043,10229058,7621962,RAL9016 Verkehrsweiß ,6.5,http://www.trilux.com/TOC/7621962,I,IP20,ETDD8,LED,68,80,70 92 99 100 100,5300,6500,TRILUX_RAL9016,TRILUX_WH_6500,Creavo_LS : TX195453
