,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SEO_2##OTHER##,Light Source##OTHER##
SFlow D1-L MRWD LED3200-840 ETDD 01,1.132,0.084,0.045,10141042,6895451,MRWD,Verkehrsweiß RAL 9016,3.3,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6895451,Schutzklasse I,IP20,ETDD,LED,26,80,3199,4000,TRILUX_Alu_RAL_9016,TRILUX_SFlow_4000,TRILUX_SFlow_4000_outer,Solvan Flow_D_LS : TX050963
