,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
ViaCon HQ-SBxL5-LRA/2600-740 4G1S ET,1.022,0.18,0.292,10158516,6997140,DB703 Anthrazit,9,http://www.trilux.com/TOC/6997140,II,IP66,ET,LED,21,70,34 70 93 99 100 11 33 56 1,2600,4000,TRILUX_DB703,TRILUX_WH_4000,ViaCon_LS : TX054653
