,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SupEqui_Mat##OTHER##,SupEqui##OTHER##,Light Source##OTHER##
Solegra D3 OTA 13500-840 ETDD + D3 ZP 01,0.9,0,0.12,10173846 + 10176493,7137951 + 7171800,RAL9016 Verkehrsweiss + RAL9016 Verkehrsweiss,13.05,http://www.trilux.com/TOC/7137951,I,IP40 + IP20,ETDD,LED,89,80,46 78 95 95 100 45 77 94 5,11700,4000,TRILUX_RAL9016,TRILUX_WH_4000_opak,TRILUX_RAL9016,Solegra_D3_ZP : 01,Solegra_LS : TX062787
