,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Aviella C09 OA 2600-830 ET 01,0.3,0,0.025,10223868,7571140,RAL9016 Verkehrsweiß,0.9,http://www.trilux.com/TOC/7571140,II,IP44,ET,LED,30,80,48 80 96 100 100 0 0 0 0,2550,3000,TRILUX_RAL9016,TRILUX_WH_3000,Aviella_LS : TX150379
Aviella C09 OA 2600-830 ETDD 01,0.3,0,0.025,10223869,7571151,RAL9016 Verkehrsweiß,0.9,http://www.trilux.com/TOC/7571151,II,IP44,ETDD,LED,30,80,48 80 96 100 100 0 0 0 0,2550,3000,TRILUX_RAL9016,TRILUX_WH_3000,Aviella_LS : TX150379
Aviella C09 OA 2600-840 ET 01,0.3,0,0.025,10223866,7571040,RAL9016 Verkehrsweiß,0.9,http://www.trilux.com/TOC/7571040,II,IP44,ET,LED,30,80,48 80 96 100 100 0 0 0 0,2750,3000,TRILUX_RAL9016,TRILUX_WH_3000,Aviella_LS : TX150378
Aviella C09 OA 2600-840 ETDD 01,0.3,0,0.025,10223867,7571051,RAL9016 Verkehrsweiß,0.9,http://www.trilux.com/TOC/7571051,II,IP44,ETDD,LED,30,80,48 80 96 100 100 0 0 0 0,2750,3000,TRILUX_RAL9016,TRILUX_WH_3000,Aviella_LS : TX150378
