,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Light Source##OTHER##,SEO##OTHER##,Mat##OTHER##,Ref##OTHER##,rotatable##OTHER##
8521 RBS3L/1000-green 1G1 ET 05,0.212,0,0.266,10130080,6491540,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6491540,Schutzklasse I,IP68,ET,LED,19,,999,green,Lutera_LS : TX046279,TRILUX_WH_green_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RBS3L/1200-830 1G1 ET 05,0.212,0,0.266,10121591,6379440,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6379440,Schutzklasse I,IP68,ET,LED,16,80,1199,3000,Lutera_LS : TX041469,TRILUX_WH_3000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RBS3L/1350-840 1G1 ET 05,0.212,0,0.266,10121590,6379340,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6379340,Schutzklasse I,IP68,ET,LED,16,80,1348,4000,Lutera_LS : TX041470,TRILUX_WH_4000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RBS3L/300-blue 1G1 ET 05,0.212,0,0.266,10130077,6491240,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6491240,Schutzklasse I,IP68,ET,LED,18,,300,blue,Lutera_LS : TX046280,TRILUX_WH_blue_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RBS3L/600-amber 1G1 ET 05,0.212,0,0.266,10130079,6491440,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6491440,Schutzklasse I,IP68,ET,LED,13,,599,amber,Lutera_LS : TX046281,TRILUX_WH_amber_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RBS3L/600-red 1G1 ET 05,0.212,0,0.266,10130078,6491340,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6491340,Schutzklasse I,IP68,ET,LED,13,,599,red,Lutera_LS : TX046282,TRILUX_WH_red_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RBS3L/600-RGB 1G1 ET 05,0.212,0,0.266,10130171,6498540,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6498540,Schutzklasse I,IP68,ET,LED,14,,599,6500,Lutera_LS : TX046283,TRILUX_WH_RGB_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RE2R/1800-830 1G1 ET,0.212,0,0.266,10121592,6379540,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6379540,Schutzklasse I,IP68,ET,LED,20,80,1799,3000,Lutera_LS : TX041471,TRILUX_WH_3000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-LED,0
8521 RE2R/2400-830 1G1 ET,0.212,0,0.266,10121596,6379940,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6379940,Schutzklasse I,IP68,ET,LED,26,80,2399,3000,Lutera_LS : TX041472,TRILUX_WH_3000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-LED,0
8521 RE2R/2900-840 1G1 ET,0.212,0,0.266,10121595,6379840,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6379840,Schutzklasse I,IP68,ET,LED,26,80,2898,4000,Lutera_LS : TX041473,TRILUX_WH_4000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-LED,0
8521 RES2L/1200-green 1G1 ET 05,0.212,0,0.266,10130072,6490740,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6490740,Schutzklasse I,IP68,ET,LED,19,,1198,green,Lutera_LS : TX046284,TRILUX_WH_green_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RES2L/1500-830 1G1 ET 05,0.212,0,0.266,10121587,6379040,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6379040,Schutzklasse I,IP68,ET,LED,16,80,1497,3000,Lutera_LS : TX041474,TRILUX_WH_3000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RES2L/1650-840 1G1 ET 05,0.212,0,0.266,10016116,4331040,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=4331040,Schutzklasse I,IP68,ET,LED,16,80,1647,4000,Lutera_LS : TX044450,TRILUX_WH_4000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RES2L/350-blue 1G1 ET 05,0.212,0,0.266,10130069,6490440,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6490440,Schutzklasse I,IP68,ET,LED,18,,349,blue,Lutera_LS : TX046285,TRILUX_WH_blue_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RES2L/750-amber 1G1 ET 05,0.212,0,0.266,10130071,6490640,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6490640,Schutzklasse I,IP68,ET,LED,13,,749,amber,Lutera_LS : TX046286,TRILUX_WH_amber_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RES2L/750-red 1G1 ET 05,0.212,0,0.266,10130070,6490540,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6490540,Schutzklasse I,IP68,ET,LED,13,,749,red,Lutera_LS : TX046287,TRILUX_WH_red_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RES2L/800-RGB 1G1 ET 05,0.212,0,0.266,10130169,6498340,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6498340,Schutzklasse I,IP68,ET,LED,14,,799,6500,Lutera_LS : TX046288,TRILUX_WH_RGB_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RM2R/1800-830 1G1 ET,0.212,0,0.266,10121594,6379740,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6379740,Schutzklasse I,IP68,ET,LED,20,80,1799,3000,Lutera_LS : TX041475,TRILUX_WH_3000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-LED,0
8521 RM2R/2000-840 1G1 ET,0.212,0,0.266,10121593,6379640,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6379640,Schutzklasse I,IP68,ET,LED,20,80,1998,4000,Lutera_LS : TX041476,TRILUX_WH_4000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-LED,0
8521 RM2R/2400-830 1G1 ET,0.212,0,0.266,10121598,6380140,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6380140,Schutzklasse I,IP68,ET,LED,26,80,2398,3000,Lutera_LS : TX041477,TRILUX_WH_3000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-LED,0
8521 RM2R/2900-840 1G1 ET,0.212,0,0.266,10121597,6380040,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6380040,Schutzklasse I,IP68,ET,LED,26,80,2898,4000,Lutera_LS : TX041478,TRILUX_WH_4000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-LED,0
8521 RMS1L/1200-green 1G1 ET 05,0.212,0,0.266,10130076,6491140,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6491140,Schutzklasse I,IP68,ET,LED,19,,1198,green,Lutera_LS : TX046289,TRILUX_WH_green_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RMS1L/1350-830 1G1 ET 05,0.212,0,0.266,10121589,6379240,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6379240,Schutzklasse I,IP68,ET,LED,16,80,1347,3000,Lutera_LS : TX041479,TRILUX_WH_3000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RMS1L/1500-840 1G1 ET 05,0.212,0,0.266,10121588,6379140,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6379140,Schutzklasse I,IP68,ET,LED,16,80,1497,4000,Lutera_LS : TX041480,TRILUX_WH_4000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RMS1L/330-blue 1G1 ET 05,0.212,0,0.266,10130073,6490840,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6490840,Schutzklasse I,IP68,ET,LED,18,,329,blue,Lutera_LS : TX046290,TRILUX_WH_blue_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RMS1L/700-amber 1G1 ET 05,0.212,0,0.266,10130075,6491040,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6491040,Schutzklasse I,IP68,ET,LED,13,,699,amber,Lutera_LS : TX046291,TRILUX_WH_amber_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RMS1L/700-red 1G1 ET 05,0.212,0,0.266,10130074,6490940,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6490940,Schutzklasse I,IP68,ET,LED,13,,699,red,Lutera_LS : TX046292,TRILUX_WH_red_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RMS1L/700-RGB 1G1 ET 05,0.212,0,0.266,10130170,6498440,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6498440,Schutzklasse I,IP68,ET,LED,14,,699,6500,Lutera_LS : TX046293,TRILUX_WH_RGB_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 AM/35HIT K,0.212,0,0.266,10016140,4333402,Tiefschwarz RAL 9005,4.6,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=4333402,Schutzklasse I,IP68,KOMP,1 x HIT-CE 35 W,48,80,634,3000,Lutera_LS : TX034765,TRILUX_WH_3000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : AM,0
8521 AM/70HIT K,0.212,0,0.266,10016141,4333502,Tiefschwarz RAL 9005,5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=4333502,Schutzklasse I,IP68,KOMP,1 x HIT 70 W,84,80,1267,3000,Lutera_LS : TX034766,TRILUX_WH_3000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : AM,0
8521 RB/TCT26/32 E (tc-t..26W),0.212,0,0.266,10016142,4333604,Tiefschwarz RAL 9005,3.7,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=4333604,Schutzklasse I,IP68,E,1 x TC-TEL 26 W,28,80,755,2700,Lutera_LS : TX034764,TRILUX_WH_2700_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : RB,0
8521 RB/TCT26/32 E (tc-t..32W),0.212,0,0.266,10016142,4333604,Tiefschwarz RAL 9005,3.7,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=4333604,Schutzklasse I,IP68,E,1 x TC-TEL 32 W,35,80,1007,2700,Lutera_LS : TX034761,TRILUX_WH_2700_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : RB,0
8521 RBS/70HST-DE K,0.212,0,0.266,10016139,4333302,Tiefschwarz RAL 9005,5.4,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=4333302,Schutzklasse I,IP68,KOMP,1 x HST-DE 70 W,83,40,4392,2000,Lutera_LS : TX034768,TRILUX_WH_2000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : RBS,1
8521 RE2R/2000-840 1G1 ET,0.212,0,0.266,10111402,6285240,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6285240,Schutzklasse I,IP68,ET,LED,20,80,1999,4000,Lutera_LS : TX039666,TRILUX_WH_4000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-LED,0
8521 RES/20HIT E,0.212,0,0.266,10072159,5935104,Tiefschwarz RAL 9005,4,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=5935104,Schutzklasse I,IP68,E,1 x HIT-CE 20 W,33,80,1532,3000,Lutera_LS : TX034781,TRILUX_WH_3000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : RES,1
8521 RES/35HIT K,0.212,0,0.266,10016135,4332902,Tiefschwarz RAL 9005,4.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=4332902,Schutzklasse I,IP68,KOMP,1 x HIT-CE 35 W,48,80,2974,3000,Lutera_LS : TX034782,TRILUX_WH_3000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : RES,1
8521 RES/70HIT K,0.212,0,0.266,10016137,4333102,Tiefschwarz RAL 9005,5.3,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=4333102,Schutzklasse I,IP68,KOMP,1 x HIT 70 W,84,80,5949,3000,Lutera_LS : TX034787,TRILUX_WH_3000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : RES,1
8521 RES/LED-B ET-B,0.212,0,0.266,10016114,4330840,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=4330840,Schutzklasse I,IP68,ED,LED,18,,136,blue,Lutera_LS : TX034788,TRILUX_WH_blue_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RES/LED-G ET-G,0.212,0,0.266,10016118,4331240,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=4331240,Schutzklasse I,IP68,ET,LED,18,,443,green,Lutera_LS : TX034791,TRILUX_WH_green_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RES/LED-R ET-R,0.212,0,0.266,10016117,4331140,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=4331140,Schutzklasse I,IP68,ET,LED,17,,299,red,Lutera_LS : TX034792,TRILUX_WH_red_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-S_LED,1
8521 RMS/35HIT K,0.212,0,0.266,10016136,4333002,Tiefschwarz RAL 9005,4.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=4333002,Schutzklasse I,IP68,KOMP,1 x HIT-CE 35 W,48,80,1915,3000,Lutera_LS : TX034789,TRILUX_WH_3000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : RMS,1
8521 RMS/70HIT K,0.212,0,0.266,10016138,4333202,Tiefschwarz RAL 9005,5.3,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=4333202,Schutzklasse I,IP68,KOMP,1 x HIT 70 W,84,80,3830,3000,Lutera_LS : TX034790,TRILUX_WH_3000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : RMS,1
