,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SupEqui_Mat##OTHER##,SupEqui##OTHER##,Light Source##OTHER##
Solegra WD2 OTA 6000-840 ET EB3 + WD2 ZP 05,0.6,0,0.12,10173802 + 10176492,7135540 + 7171700,RAL9016 Verkehrsweiss + RAL9005 Tiefschwarz,7.4,http://www.trilux.com/TOC/7135540,I,IP40 + IP20,ET,LED,48,80,46 78 95 95 100 45 77 94 5,5300,4000,TRILUX_RAL9016,TRILUX_WH_4000_opak,TRILUX_RAL9005,Solegra_WD2_ZP : 05,Solegra_LS : TX062920
