,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Acquex LED-M 6 20-830 ET PC IX,0.665,0.145,0.101,10254440,7910940,RAL1003 Signalgelb,1.516,http://www.trilux.com/TOC/7910940,I,IP66,ET,LED,18,80,36 64 85 89 100 2 9 22 11,2200,3000,TRILUX_RAL1003 Signalgelb,TRILUX_WH_3000,Acquex_LS : TX279601
