,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Opendo D2-L DWW 52-840 ET 01,1.408,0.161,0.045,10240288,7746140,RAL9016 Verkehrsweiß ,4.7,http://www.trilux.com/TOC/7746140,I,IP20,ET,LED,35,80,50 83 97 100 100,5200,4000,TRILUX_RAL9016,TRILUX_WH_4000,Opendo_LS : TX277472
