,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SEO_outer##OTHER##,cutout_radius##LENGTH##METERS,Light Source##OTHER##
Inplana C09 OTA22 2000-830 ETDD 01 + C09 ZPF-T-T,0.316,0,0.0417,10126204,6455351,Inplana_C09 : Inplana_C09_ZPF-T,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455351,Schutzklasse II,,ETDD,LED,18,80,1900,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.163,Inplana_LS : TX045475
