,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
LnStar 40-RB2L/7500-740 8G1S ET,0.523,0.29,0.116,10145866,6903840,RAL9006 Weißaluminium,7,http://www.trilux.com/TOC/6903840,I,IP66,ET,LED,54,70,88 96 99 100 100,7500,4000,TRILUX_RAL9006,TRILUX_WH_4000,LnStar_40_LS : TX054210
