,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Ref##OTHER##,WW##OTHER##,Light Source##OTHER##
InperlaL G2 C07 BR19 2700-840 ETDD 03 + RD-PC,0.235,0,0.105,10143923;10143987;,6868451;6871500;,InperlaL_C07_RD-PC,RAL9006 Weißaluminium;,1.125,http://www.trilux.com/TOC/6868451,Schutzklasse I,IP40,ETDD,LED,25,80,86 97 99 100 100 40 80 80 0,2699,4000,TRILUX_Alu_RAL_9006,TRILUX_WH_4000_InperlaL,TRILUX_BR_InperlaL,0,InperlaL_C07_LS : TX052854
