,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
OleveonF 15 L 27-75/16 ML-840 ET (Stage D),1.552,0.102,0.091,10229806,7663740,RAL7035 Lichtgrau,2.5,http://www.trilux.com/TOC/7663740,I,IP66,ET,LED,54,80,47 76 92 94 100 4 9 34 6,7500,4000,TRILUX_RAL7035,TRILUX_WH_4000,OleveonF_LS : TX194530
