,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Ref##OTHER##,Light Source##OTHER##
InperlaLP C05 BR19 1000-840 ETDD 03 + RG-PC,0.15,0,0.105,10117482,6355251,InperlaLP_RG-PC,RAL9006 Weißaluminium,1.317,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6355251,Schutzklasse I,IP20,ETDD,LED,10,80,88 96 99 100 100,999,4000,TRILUX_Alu_RAL_9006,TRILUX_WH_4000_InperlaLP,TRILUX_BR_InperlaLP,InperlaLP_LS : TX041502
