,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Ref##OTHER##,WW##OTHER##,Light Source##OTHER##
InperlaL G2 C07 BR19 1800-840 ET 01,0.235,0,0.1,10143893;,6867040;,InperlaL_no_accessories,RAL9016 Verkehrsweiß;,1,http://www.trilux.com/TOC/6867040,Schutzklasse II,IP40,ET,LED,16,80,90 100 100 100 100,1799,4000,TRILUX_Alu_RAL_9016,TRILUX_WH_4000_InperlaL,TRILUX_BR_InperlaL,0,InperlaL_C07_LS : TX052570
