,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Lutera 100 C RM4L/1000-830 1G1P ET,0.152,0.152,0.08,10158158,6967440,Edelstahl,1,http://www.trilux.com/TOC/6967440,II,IP68,ET,LED,11,80,94 99 100 100 100,1000,3000,TRILUX_Edelstahl,TRILUX_WH_3000,Lutera_LS : TX054498
