,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Solegra WD2 OTA 6000-830 ET + WD2 ZP C1/C,0.6,0,0.12,10173800 + 10173933,7135340 + 7132100,RAL9016 Verkehrsweiss + RAL9016 Verkehrsweiss,9.3,http://www.trilux.com/TOC/7135340,I,IP40 + IP20,ET,LED,43,80,46 78 95 100 100,4800,3000,TRILUX_RAL9016,TRILUX_WH_3000_opak,Solegra_LS : TX062809
