,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
LTX P-AB2L-LR/3800-730 4G1 ET,0.57,0,0.606,10169198,7082740,DB703 Anthrazit,7.54,http://www.trilux.com/TOC/7082740,II,IP65,ET,LED,39,70,24 61 92 100 100 0 0 0 0,3800,3000,TRILUX_DB703,TRILUX_WH_3000,Lumantix_LS : TX055902
