,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Opendo D2-L PW19 47-840 ETDD +CO2 01,1.408,0.161,0.045,10242246,7764751,RAL9016 Verkehrsweiß ,4.9,http://www.trilux.com/TOC/7764751,I,IP20,ETDD,LED,37,80,65 90 98 99 100 14 43 71 1,4700,4000,TRILUX_RAL9016,TRILUX_WH_4000,Opendo_LS : TX277520
