,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SupEqui##OTHER##,Light Source##OTHER##
Solegra D3 OTA 13500-840 ETDD + ZS DB 5075/3000,0.9,0,0.12,10173846 + 10173928,7137951 + 7131600,RAL9016 Verkehrsweiss + RAL9016 Verkehrsweiss,13.5,http://www.trilux.com/TOC/7137951,I,IP40 + IP20,ETDD,LED,89,80,44 75 93 89 100 25 52 77 11,13500,4000,TRILUX_RAL9016,TRILUX_WH_4000_opak,Solegra_D3_ZS_DB : 5075/3000,Solegra_LS : TX062895
