,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
OleveonF 1.5 L 4000-865 ET,1.552,0.102,0.091,10173617,7124740,RAL7035 Lichtgrau,2.5,http://www.trilux.com/TOC/7124740,I,IP66,ET,LED,32,80,50 81 94 94 100 0 2 39 6,4000,6500,TRILUX_RAL7035 ,TRILUX_WH_6500,OleveonF_LS : TX056135
