,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SEO_outer##OTHER##,cutout_radius##LENGTH##METERS,Light Source##OTHER##
Inplana C07 OTA22 1000-830 ET 01 + C07 ZPF-T-T,0.234,0,0.0417,10130563,6454740,Inplana_C07 : Inplana_C07_ZPF-T,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454740,Schutzklasse II,,ET,LED,"9,5",80,1200,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.123,Inplana_LS : TX045465
