,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,SupEqui##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
SFlow H2-L LW19 6400-840 ETDD 01,1.413,0.084,0.045,10225288,7573651,RAL9016 Verkehrsweiß,4.2,http://www.trilux.com/TOC/7573651,I,IP20,ETDD,LED,43,80,80 96 99 99 100 27 64 91 1,6400,4000,H-L_LW19,TRILUX_RAL9016,TRILUX_WH_4000,SFlow_H_LS : TX150318
