,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SEO_outer##OTHER##,cutout_radius##LENGTH##METERS,Light Source##OTHER##
Inplana C09 OTA22 2000-830 ETDD 01 + C09 ZPF - T,0.316,0,0.041,10126204+10126346,6455351+6456400,Inplana_C09 : Inplana_C09_ZPF-T,RAL9016 Verkehrsweiß,2.83,http://www.trilux.com/TOC/6455351,IIII,IP20,ETDD,LED,15,80,52 83 96 100 100 0 0 0 0,1900,3000,TRILUX_RAL9016,TRILUX_WH_3000,TRILUX_CDP_Inplana_WH_outer_3000,0.163,Inplana_LS : TX045475
