,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Lunexo D1 CDP-I 4400 830 ETDD +LLWC 01,1.203,0.2,0.049,10143030;,6828751;,Lunexo_D_GH,Verkehrsweiß RAL 9016;,8.5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6828751,Schutzklasse I;,IP20;,ETDD,LED,47,80,4.199,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_3000_Lunexo,Lunexo_LS : TX051300
Lunexo D1 CDP-I 4400 830 ETDD +LLWM 01,1.203,0.2,0.049,10143028;,6828551;,Lunexo_D_GH,Verkehrsweiß RAL 9016;,8.5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6828551,Schutzklasse I;,IP20;,ETDD,LED,47,80,4.199,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_3000_Lunexo,Lunexo_LS : TX051301
Lunexo D1 CDP-I 4400 830 ETDD 01,1.203,0.2,0.049,10143020;,6827751;,Lunexo_D_GH,Verkehrsweiß RAL 9016;,8.5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6827751,Schutzklasse I;,IP20;,ETDD,LED,47,80,4.199,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_3000_Lunexo,Lunexo_LS : TX051302
Lunexo D1 CDP-I 4400 830 ETDD 03,1.203,0.2,0.049,10143022;,6827951;,Lunexo_D_GH,Weißaluminium RAL 9006;,8.5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6827951,Schutzklasse I;,IP20;,ETDD,LED,47,80,4.199,3000,TRILUX_Alu_RAL_9006,TRILUX_PMMA_3000_Lunexo,Lunexo_LS : TX051303
Lunexo D1 CDP-I 4400 840 ETDD +LLWC 01,1.203,0.2,0.049,10143031;,6828851;,Lunexo_D_GH,Verkehrsweiß RAL 9016;,8.5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6828851,Schutzklasse I;,IP20;,ETDD,LED,47,80,4.399,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX051304
Lunexo D1 CDP-I 4400 840 ETDD +LLWM 01,1.203,0.2,0.049,10143029;,6828651;,Lunexo_D_GH,Verkehrsweiß RAL 9016;,8.5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6828651,Schutzklasse I;,IP20;,ETDD,LED,47,80,4.399,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX051305
Lunexo D1 CDP-I 4400 840 ETDD 01,1.203,0.2,0.049,10143021;,6827851;,Lunexo_D_GH,Verkehrsweiß RAL 9016;,8.5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6827851,Schutzklasse I;,IP20;,ETDD,LED,47,80,4.399,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX051306
Lunexo D1 CDP-I 4400 840 ETDD 03,1.203,0.2,0.049,10143023;,6828051;,Lunexo_D_GH,Weißaluminium RAL 9006;,9.3,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6828051,Schutzklasse I;,IP20;,ETDD,LED,47,80,4.399,4000,TRILUX_Alu_RAL_9006,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX051307
Lunexo D2 CDP-I 5500 830 ETDD +LLWC 01,1.503,0.2,0.049,10143034;,6829151;,Lunexo_D_GH,Verkehrsweiß RAL 9016;,10,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6829151,Schutzklasse I;,IP20;,ETDD,LED,58,80,5.199,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_3000_Lunexo,Lunexo_LS : TX051308
Lunexo D2 CDP-I 5500 830 ETDD +LLWM 01,1.503,0.2,0.049,10143032;,6828951;,Lunexo_D_GH,Verkehrsweiß RAL 9016;,10,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6828951,Schutzklasse I;,IP20;,ETDD,LED,58,80,5.199,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_3000_Lunexo,Lunexo_LS : TX051309
Lunexo D2 CDP-I 5500 830 ETDD 01,1.503,0.2,0.049,10143024;,6828151;,Lunexo_D_GH,Verkehrsweiß RAL 9016;,10,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6828151,Schutzklasse I;,IP20;,ETDD,LED,58,80,5.199,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_3000_Lunexo,Lunexo_LS : TX051310
Lunexo D2 CDP-I 5500 830 ETDD 03,1.503,0.2,0.049,10143026;,6828351;,Lunexo_D_GH,Weißaluminium RAL 9006;,10,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6828351,Schutzklasse I;,IP20;,ETDD,LED,58,80,5.199,3000,TRILUX_Alu_RAL_9006,TRILUX_PMMA_3000_Lunexo,Lunexo_LS : TX051311
Lunexo D2 CDP-I 5500 840 ETDD +LLWC 01,1.503,0.2,0.049,10143035;,6829251;,Lunexo_D_GH,Verkehrsweiß RAL 9016;,10,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6829251,Schutzklasse I;,IP20;,ETDD,LED,58,80,5.499,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX051312
Lunexo D2 CDP-I 5500 840 ETDD +LLWM 01,1.503,0.2,0.049,10143033;,6829051;,Lunexo_D_GH,Verkehrsweiß RAL 9016;,10,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6829051,Schutzklasse I;,IP20;,ETDD,LED,58,80,5.499,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX051313
Lunexo D2 CDP-I 5500 840 ETDD 01,1.503,0.2,0.049,10143025;,6828251;,Lunexo_D_GH,Verkehrsweiß RAL 9016;,10,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6828251,Schutzklasse I;,IP20;,ETDD,LED,58,80,5.499,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX051314
Lunexo D2 CDP-I 5500 840 ETDD 03,1.503,0.2,0.049,10143027;,6828451;,Lunexo_D_GH,Weißaluminium RAL 9006;,10,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6828451,Schutzklasse I;,IP20;,ETDD,LED,58,80,5.499,4000,TRILUX_Alu_RAL_9006,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX051315
Lunexo H1 CDP-I 6500 830 ETDD +LLWM 01,1.203,0.2,0.045,10143004;,6826151;,Lunexo_H_GH,Verkehrsweiß RAL 9016;,9,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6826151,Schutzklasse I;,IP20;,ETDD,LED,61,80,5.799,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_3000_Lunexo,Lunexo_LS : TX050906
Lunexo H1 CDP-I 6500 830 ETDD +LLWC 01,1.203,0.2,0.045,10143006;,6826351;,Lunexo_H_GH,Verkehrsweiß RAL 9016;,9,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6826351,Schutzklasse I;,IP20;,ETDD,LED,61,80,5.799,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_3000_Lunexo,Lunexo_LS : TX050907
Lunexo H1 CDP-I 6500 830 ETDD 01,1.203,0.2,0.045,10142996;,6825351;,Lunexo_H_GH,Verkehrsweiß RAL 9016;,9,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6825351,Schutzklasse I;,IP20;,ETDD,LED,61,80,5.799,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_3000_Lunexo,Lunexo_LS : TX050908
Lunexo H1 CDP-I 6500 830 ETDD 03,1.203,0.2,0.045,10142998;,6825551;,Lunexo_H_GH,Weißaluminium RAL 9006;,9,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6825551,Schutzklasse I;,IP20;,ETDD,LED,61,80,5.799,3000,TRILUX_Alu_RAL_9006,TRILUX_PMMA_3000_Lunexo,Lunexo_LS : TX050909
Lunexo H1 CDP-I 6500 840 ETDD +LLWM 01,1.203,0.2,0.045,10143005;,6826251;,Lunexo_H_GH,Verkehrsweiß RAL 9016;,9,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6826251,Schutzklasse I;,IP20;,ETDD,LED,61,80,6.099,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX050910
Lunexo H1 CDP-I 6500 840 ETDD +LLWC 01,1.203,0.2,0.045,10143007;,6826451;,Lunexo_H_GH,Verkehrsweiß RAL 9016;,9,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6826451,Schutzklasse I;,IP20;,ETDD,LED,61,80,6.099,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX050911
Lunexo H1 CDP-I 6500 840 ETDD 01,1.203,0.2,0.045,10142997;,6825451;,Lunexo_H_GH,Verkehrsweiß RAL 9016;,9.6,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6825451,Schutzklasse I;,IP20;,ETDD,LED,61,80,6.099,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX050912
Lunexo H1 CDP-I 6500 840 ETDD 03,1.203,0.2,0.045,10142999;,6825651;,Lunexo_H_GH,Weißaluminium RAL 9006;,9,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6825651,Schutzklasse I;,IP20;,ETDD,LED,61,80,6.099,4000,TRILUX_Alu_RAL_9006,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX050913
Lunexo H2 CDP-I 8800 830 ETDD +LLWM 01,1.503,0.2,0.045,10143008;,6826551;,Lunexo_H_GH,Verkehrsweiß RAL 9016;,10.5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6826551,Schutzklasse I;,IP20;,ETDD,LED,80,80,7.898,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_3000_Lunexo,Lunexo_LS : TX050914
Lunexo H2 CDP-I 8800 830 ETDD +LLWC 01,1.503,0.2,0.045,10143010;,6826751;,Lunexo_H_GH,Verkehrsweiß RAL 9016;,10.5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6826751,Schutzklasse I;,IP20;,ETDD,LED,80,80,7.898,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_3000_Lunexo,Lunexo_LS : TX050915
Lunexo H2 CDP-I 8800 830 ETDD 01,1.503,0.2,0.045,10143000;,6825751;,Lunexo_H_GH,Verkehrsweiß RAL 9016;,10.5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6825751,Schutzklasse I;,IP20;,ETDD,LED,80,80,7.898,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_3000_Lunexo,Lunexo_LS : TX050916
Lunexo H2 CDP-I 8800 830 ETDD 03,1.503,0.2,0.045,10143002;,6825951;,Lunexo_H_GH,Weißaluminium RAL 9006;,10.5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6825951,Schutzklasse I;,IP20;,ETDD,LED,80,80,7.898,3000,TRILUX_Alu_RAL_9006,TRILUX_PMMA_3000_Lunexo,Lunexo_LS : TX050917
Lunexo H2 CDP-I 8800 840 ETDD +LLWM 01,1.503,0.2,0.045,10143009;,6826651;,Lunexo_H_GH,Verkehrsweiß RAL 9016;,10.5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6826651,Schutzklasse I;,IP20;,ETDD,LED,80,80,8.298,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX050918
Lunexo H2 CDP-I 8800 840 ETDD +LLWC 01,1.503,0.2,0.045,10143011;,6826851;,Lunexo_H_GH,Verkehrsweiß RAL 9016;,10.5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6826851,Schutzklasse I;,IP20;,ETDD,LED,80,80,8.298,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX050919
Lunexo H2 CDP-I 8800 840 ETDD 01,1.503,0.2,0.045,10143001;,6825851;,Lunexo_H_GH,Verkehrsweiß RAL 9016;,10.5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6825851,Schutzklasse I;,IP20;,ETDD,LED,80,80,8.298,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX050920
Lunexo H2 CDP-I 8800 840 ETDD 03,1.503,0.2,0.045,10143003;,6826051;,Lunexo_H_GH,Weißaluminium RAL 9006;,10.5,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6826051,Schutzklasse I;,IP20;,ETDD,LED,80,80,8.298,4000,TRILUX_Alu_RAL_9006,TRILUX_PMMA_4000_Lunexo,Lunexo_LS : TX050921
