,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Ref##OTHER##,SupEqui_SEO##OTHER##,SupEqui##OTHER##,Light Source##OTHER##
SNS QC5 HRW 20-940 ETDD 01,0.165,0.165,0.13,10183601,,RAL9016 Verkehrsweiß,1.25,,I,IP20,ETDD,LED,26,90,71 95 100 100 100,2100,4000,TRILUX_RAL9016,TRILUX_WH_4000,TRILUX_HR,TRILUX_PC-T,Sonnos_QC5_W_no_accessories,Sonnos_LS : TX068756
SNS QC5 HRW 20-940 ETDD 01 + QC05 ZIP54-PC-T-T,0.165,0.165,0.13,10183601 + 10179649,7188500,RAL9016 Verkehrsweiß,1.333,,I,IP20 IP54,ETDD,LED,26,90,71 95 100 100 100,2100,4000,TRILUX_RAL9016,TRILUX_WH_4000,TRILUX_HR,TRILUX_PC-T,Sonnos_QC5_ZIP54,Sonnos_LS : TX068927
