,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,SupEqui##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
SFlow D3-L MRX LED4000-840 ETDD LLWS 01,1.473,0.084,0.045,10148048,6916351,RAL9016 Verkehrsweiß,4.3,http://www.trilux.com/TOC/6916351,I,IP20,ETDD,LED,30,80,84 99 100 100 100,4000,4000,D-L_MR_LLW,TRILUX_RAL9016,TRILUX_WH_4000,SFlow_D_LS : TX053178
