,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SEO_2##OTHER##,Light Source##OTHER##
SFlow C2-L MRWD LED4000-840 ETDD 01,1.413,0.1,0.045,10141028,6894051,MRWD,Verkehrsweiß RAL 9016,4.08,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6894051,Schutzklasse I,IP20,ETDD,LED,32,80,3999,4000,TRILUX_Alu_RAL_9016,TRILUX_SFlow_4000,TRILUX_SFlow_4000_outer,Solvan Flow_C_LS : TX050952
