,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Ref##OTHER##,WW##OTHER##,Light Source##OTHER##
InperlaL G2 C07 HR22 3800-840 ET 03 + DA-M 03,0.235,0,0.14,10143954;10143986;,6870040;6871400;,InperlaL_C07_DA : M 03,RAL9006 Weißaluminium;RAL9006 Weißaluminium;,1.66,http://www.trilux.com/TOC/6870040,Schutzklasse II,IP40,ET,LED,39,80,67 91 98 100 100,2999,4000,TRILUX_Alu_RAL_9006,TRILUX_WH_4000_InperlaL,TRILUX_HR_InperlaL,0,InperlaL_C07_LS : TX054418
