,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,Light Source##OTHER##
Nextrema G3 TB 8000-840 ETDD,1.042,0.092,0.112,10136235,6634151,Nextrema_Pmma_G3 : XB_TB,Anthrazit DB 703,3.2,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6634151,Schutzklasse I,IP66,ETDD,LED,57,80,7.998,4000,TRILUX_Alu_DB703,Nextrema_G3_LS : TX047419
