,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SEO_2##OTHER##,Light Source##OTHER##
SFlow D1-L MRX LED3200-830 ET 03,1.132,0.084,0.045,10141057,6895740,MRW_MRX : MRX,Weißaluminium RAL 9006,3.19,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6895740,Schutzklasse I,IP20,ET,LED,26,80,2999,3000,TRILUX_Alu_RAL_9006,TRILUX_SFlow_3000,TRILUX_SFlow_3000_outer,Solvan Flow_D_LS : TX050966
