,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Ref##OTHER##,WW##OTHER##,Light Source##OTHER##
InperlaL G2 C07 BR22 1800-830 ETDD 03 + DA 03,0.235,0,0.1,10143872;10143984;,6865951;6871200;,InperlaL_C07_DA : 03,RAL9006 Weißaluminium;RAL9006 Weißaluminium;,1.36,http://www.trilux.com/TOC/6865951,Schutzklasse I,IP40,ETDD,LED,16,80,75 99 100 100 100,1600,3000,TRILUX_Alu_RAL_9006,TRILUX_WH_3000_InperlaL,TRILUX_BR_InperlaL,0,InperlaL_C07_LS : TX052864
