,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##,uff##OTHER##
Bicult Act T SMC NGS 5500 ETDI 01 EU (ActCWW),0.32,0.24,0.036,10169589,7094259,RAL9016 Verkehrsweiß,1.234,http://www.trilux.com/TOC/7094259,,,ETD,LED,56,80,59 89 98 10 100 82 96 100 90,5578,2700,TRILUX_Alu_RAL_9016,Bicult_WH2700,BICULT_LS : TX056967,90
