,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
AragF 15 PW 44-840 ETDD +LLWRR PC,1.552,0.102,0.091,10204917,7409051,RAL7035 Lichtgrau,3.2,http://www.trilux.com/TOC/7409051,I,IP66,ETDD,LED,28,80,56 85 95 93 100 0 0 11 7,4300,4000,TRILUX_RAL7035,TRILUX_WH_4000,Aragon_Fit_LS : TX112851
