,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,SupEqui##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
SFlow H2-L CDP-I 6300-830 ET 01,1.413,0.1,0.07,10198455,7358440,RAL9016 Verkehrsweiß,4.55,http://www.trilux.com/TOC/7358440,I,IP20,ET,LED,52,80,66 88 96 62 100 40 71 91 38,6300,3000,H-L_CDP,TRILUX_RAL9016,TRILUX_WH_3000,SFlow_H_LS : TX133395
