,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Sanesca W1 LED2000-840 ETDD 03,0.7,0.19,0.09,10117154,6337351,1,Weißaluminium RAL 9006,4,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6337351,Schutzklasse I,,ETDD,LED,20,80,2000,4000,TRILUX_Alu_RAL_9006,TRILUX_PMMA_4000_Sanesca,Sanesca_LS : TX040694
