,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Ref##OTHER##,SupEqui_SEO##OTHER##,SupEqui##OTHER##,Light Source##OTHER##
SNS RC7 HRW 20-940 ETDD 01,0.228,0,0.127,10183454,,RAL9016 Verkehrsweiß,1.61,,I,IP20,ETDD,LED,26,90,68 94 100 100 100,2000,4000,TRILUX_RAL9016,TRILUX_WH_4000,TRILUX_HR,TRILUX_PC-T,Sonnos_RC7_W_no_accessories,Sonnos_LS : TX068817
SNS RC7 HRW 20-940 ETDD 01 + RC07 ZIP54-PC-T-T,0.228,0,0.127,10183454 + 10179652,7188800,RAL9016 Verkehrsweiß,1.737,,I,IP20 IP54,ETDD,LED,26,90,68 94 100 100 100,2000,4000,TRILUX_RAL9016,TRILUX_WH_4000,TRILUX_HR,TRILUX_PC-T,Sonnos_RC7_ZIP54,Sonnos_LS : TX068984
