,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
FidescaBS G3 M57 DL 75-840 ETDD,1.247,0.309,0.094,10234335,7687451,RAL9016 Verkehrsweiß,6.7,http://www.trilux.com/TOC/7687451,I,IP54,ETDD,LED,54,80,53 84 97 100 100 0 0 0 0,7500,4000,TRILUX_RAL9016,TRILUX_WH_4000,FidescaBS_G3_LS : TX200006
