,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SupEqui_Mat##OTHER##,SupEqui##OTHER##,Light Source##OTHER##
Solegra WD2 OTA 6000-830 ETDD + WD2 ZP CDP 03,0.61,0,0.12,10173804 + 10181234,7135351 + 7208100,RAL9016 Verkehrsweiss + RAL9006 Weissaluminium,8.1,http://www.trilux.com/TOC/7135351,I,IP40 + IP20,ETDD,LED,43,80,57 86 97 91 100 42 72 91 9,4000,3000,TRILUX_RAL9016,TRILUX_WH_3000_opak,TRILUX_RAL9006,Solegra_WD2_ZP_CDP : 03,Solegra_LS : TX068365
