,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Light Source##OTHER##,SEO##OTHER##,Mat##OTHER##,Ref##OTHER##,rotatable##OTHER##
8521 RE2R/1800-830 1G1 ET,0.212,0,0.266,10121592,6379540,Tiefschwarz RAL 9005,3.8,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6379540,Schutzklasse I,IP68,ET,LED,20,80,1799,3000,Lutera_LS : TX041471,TRILUX_WH_3000_Lutera,TRILUX_Alu_RAL 9005,Lutera_200_ref : R-LED,0
