,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SEO_outer##OTHER##,cutout_radius##LENGTH##METERS,Light Source##OTHER##
Inplana C07 OTA22 1000-840 ETDD 01 + C07 ZPF - T WR,0.235,0,0.041,10126197+10126341,6454651+6455900,Inplana_C07 : Inplana_C07_ZPF-T_WR,RAL9016 Verkehrsweiß,2.24,http://www.trilux.com/TOC/6454651,IIII,IP20,ETDD,LED,9,80,52 83 96 100 100 0 0 0 0,1200,4000,TRILUX_RAL9016,TRILUX_WH_4000,TRILUX_CDP_Inplana_WH_outer_4000,0.163,Inplana_LS : TX045468
