,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
Opendo H2-L PW19 64-830 ETDD +LLWM 03,1.408,0.161,0.045,10242272,7766951,RAL9006 Weißaluminium ,5.1,http://www.trilux.com/TOC/7766951,I,IP20,ETDD,LED,54,80,65 90 98 71 100 32 64 88 29,6100,3000,TRILUX_RAL9006,TRILUX_WH_3000,Opendo_LS : TX277413
