,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Ref##OTHER##,Light Source##OTHER##
SNS QD7 MRVFL-19 26-840 ETDD 01,0.206,0.206,0.175,10183648,,RAL9016 Verkehrsweiß,3.1,,I,IP20,ETDD,LED,23,80,95 100 100 100 100,2600,4000,TRILUX_RAL9016,TRILUX_WH_4000,TRILUX_MR,Sonnos_LS : TX068780
SNS QD7 MRVFL-19 26-840 ETDD 05,0.206,0.206,0.175,10183647,,RAL9005 Tiefschwarz,3.1,,I,IP20,ETDD,LED,23,80,95 100 100 100 100,2600,4000,TRILUX_RAL9005,TRILUX_WH_4000,TRILUX_MR,Sonnos_LS : TX068781
SNS QH7-2Q MRVFL-19 26-840 ETDD 01,0.206,0.206,0.175,10183035,,RAL9016 Verkehrsweiß,3.86,,I,IP20,ETDD,LED,23,80,95 100 100 100 100,2600,4000,TRILUX_RAL9016,TRILUX_WH_4000,TRILUX_MR,Sonnos_LS : TX068784
SNS QH7-2Q MRVFL-19 26-840 ETDD 05,0.206,0.206,0.175,10183034,,RAL9005 Tiefschwarz,3.86,,I,IP20,ETDD,LED,23,80,95 100 100 100 100,2600,4000,TRILUX_RAL9005,TRILUX_WH_4000,TRILUX_MR,Sonnos_LS : TX068785
