,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
OleveonF 12 L 21-66/16 ML-840 ET (Stage A),1.257,0.102,0.091,10229802,7663340,RAL7035 Lichtgrau,2,http://www.trilux.com/TOC/7663340,I,IP66,ET,LED,36,80,47 76 92 94 100 4 9 34 6,5200,4000,TRILUX_RAL7035,TRILUX_WH_4000,OleveonF_LS : TX194513
