,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,Light Source##OTHER##
OleveonF 1.5 B 4000-840 ETDD PC+LV,1.552,0.102,0.091,10173581,7122051,RAL7035 Lichtgrau,2.8,http://www.trilux.com/TOC/7122051,I,IP66,ETDD,LED,28,80,56 85 95 93 100 0 0 11 7,3900,4000,TRILUX_RAL7035 ,TRILUX_WH_4000,OleveonF_LS : TX056196
