,l##LENGTH##METERS,w##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,PrimEqui##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,MatSupEqui##OTHER##,SEO##OTHER##,Light Source##OTHER##
ArimoFit M73 PW19 42-840 ET,0.597,0.597,0.02,10207408,7528740,ArimoFit_M46_ M48_M57_M59_M73_M84,ArimoFit_no_accessories,RAL9016 Verkehrsweiß,3.4,http://www.trilux.com/TOC/7528740,II,IP40,ET,LED,31,80,64 89 97 100 100 0 0 0 0,4200,4000,TRILUX_RAL9016,TRILUX_RAL9016,TRILUX_WH_4000,ArimoFit_LS : TX149973
