,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,CENFluxCode##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO_1##OTHER##,SEO_2##OTHER##,Light Source##OTHER##
Skeo Q-W2 GT AE2R/70-830 ETDD,0.15,0.15,0.15,10184839,7232751,DB703 Anthrazit,2.8,http://www.trilux.com/TOC/7232751,I,IP65,ETDD,LED,9,80,99 99 100 100 96,70,3000,TRILUX_RAL703,TRILUX_WH_3000_transp,TRILUX_WH_3000,Skeo_Q_LS : TX076385
